**Microprocessor**

**Liquid Crystal Display (LCD)**

**Monitor (GUI)**

**Pseudo RFID (Keypad)**

Display “Tap any key to start”

Displays “Tap Cash Card” @ LCD

Swaps to Tap Cash Card Screen

Microprocessor awaits keypad input

Return to Main Menu

Interrupts that time to scan cash card is up

30 Second Delay